
                                     
Adapter #2

==============================================================================
                    Versions
                ================
Product Name    : ServeRAID M5225
Serial No       : SV43328814
FW Package Build: 24.2.1-0052

                    Mfg. Data
                ================
Mfg. Date       : 08/19/14
Rework Date     : 00/00/00
Revision No     : 04A
Battery FRU     : N/A

                Image Versions in Flash:
                ================
BIOS Version       : B6.14.05.4_4.16.08.00_0xB603050
Ctrl-R Version     : 5.03-0005
Preboot CLI Version: 01.07-05:#%0000
FW Version         : 4.220.120-3749
NVDATA Version     : 3.1310.00-0080
Boot Block Version : 3.02.00.00-0000

                Pending Images in Flash
                ================
None

                PCI Info
                ================
Controller Id	: 0000
Vendor Id       : 1000
Device Id       : 005d
SubVendorId     : 1014
SubDeviceId     : 0455

Host Interface  : PCIE

ChipRevision    : C0

Link Speed 	     : 0 
Number of Frontend Port: 0 
Device Interface  : PCIE

Number of Backend Port: 8 
Port  :  Address
0        500c0ff026449f3f 
1        500c0ff02649463f 
2        0000000000000000 
3        0000000000000000 
4        0000000000000000 
5        0000000000000000 
6        0000000000000000 
7        0000000000000000 

                HW Configuration
                ================
SAS Address      : 500605b009352a70
BBU              : Absent
Alarm            : Absent
NVRAM            : Present
Serial Debugger  : Present
Memory           : Present
Flash            : Present
Memory Size      : 2048MB
TPM              : Absent
On board Expander: Absent
Upgrade Key      : Absent
Temperature sensor for ROC    : Present
Temperature sensor for controller    : Absent

ROC temperature : 71  degree Celcius

                Settings
                ================
Current Time                     : 17:37:41 12/10, 2015
Predictive Fail Poll Interval    : 65535sec
Interrupt Throttle Active Count  : 16
Interrupt Throttle Completion    : 50us
Rebuild Rate                     : 100%
PR Rate                          : 0%
BGI Rate                         : 100%
Check Consistency Rate           : 0%
Reconstruction Rate              : 100%
Cache Flush Interval             : 4s
Max Drives to Spinup at One Time : 2
Delay Among Spinup Groups        : 12s
Physical Drive Coercion Mode     : 1GB
Cluster Mode                     : Disabled
Alarm                            : Disabled
Auto Rebuild                     : Enabled
Battery Warning                  : Enabled
Ecc Bucket Size                  : 15
Ecc Bucket Leak Rate             : 1440 Minutes
Restore HotSpare on Insertion    : Disabled
Expose Enclosure Devices         : Enabled
Maintain PD Fail History         : Enabled
Host Request Reordering          : Enabled
Auto Detect BackPlane Enabled    : SGPIO/i2c SEP
Load Balance Mode                : Auto
Use FDE Only                     : Yes
Security Key Assigned            : No
Security Key Failed              : No
Security Key Not Backedup        : No
Default LD PowerSave Policy      : Controller Defined
Maximum number of direct attached drives to spin up in 1 min : 10 
Auto Enhanced Import             : Yes
Any Offline VD Cache Preserved   : No
Allow Boot with Preserved Cache  : No
Disable Online Controller Reset  : No
PFK in NVRAM                     : Yes
Use disk activity for locate     : No
POST delay			 : 90 seconds
BIOS Error Handling          	 : Stop On Errors
Current Boot Mode 		  :Normal
                Capabilities
                ================
RAID Level Supported             : RAID0, RAID1, RAID5, RAID00, RAID10, RAID50, PRL 11, PRL 11 with spanning, SRL 3 supported, PRL11-RLQ0 DDF layout with no span, PRL11-RLQ0 DDF layout with span
Supported Drives                 : SAS, SATA

Allowed Mixing:

Mix in Enclosure Allowed

                Status
                ================
ECC Bucket Count                 : 0

                Limitations
                ================
Max Arms Per VD          : 32 
Max Spans Per VD         : 8 
Max Arrays               : 128 
Max Number of VDs        : 64 
Max Parallel Commands    : 928 
Max SGE Count            : 60 
Max Data Transfer Size   : 8192 sectors 
Max Strips PerIO         : 42 
Max LD per array         : 64 
Min Strip Size           : 64 KB
Max Strip Size           : 1.0 MB
Max Configurable CacheCade Size: 0 GB
Current Size of CacheCade      : 0 GB
Current Size of FW Cache       : 1737 MB

                Device Present
                ================
Virtual Drives    : 1 
  Degraded        : 0 
  Offline         : 0 
Physical Devices  : 20 
  Disks           : 17 
  Critical Disks  : 0 
  Failed Disks    : 0 

                Supported Adapter Operations
                ================
Rebuild Rate                    : Yes
CC Rate                         : Yes
BGI Rate                        : Yes
Reconstruct Rate                : Yes
Patrol Read Rate                : Yes
Alarm Control                   : No
Cluster Support                 : No
BBU                             : Yes
Spanning                        : Yes
Dedicated Hot Spare             : Yes
Revertible Hot Spares           : Yes
Foreign Config Import           : Yes
Self Diagnostic                 : Yes
Allow Mixed Redundancy on Array : No
Global Hot Spares               : Yes
Deny SCSI Passthrough           : No
Deny SMP Passthrough            : No
Deny STP Passthrough            : No
Support Security                : No
Snapshot Enabled                : No
Support the OCE without adding drives : Yes
Support PFK                     : Yes
Support PI                      : Yes
Support Boot Time PFK Change    : Yes
Disable Online PFK Change       : Yes
Support LDPI Type1                      : No
Support LDPI Type2                      : No
Support LDPI Type3                      : No
PFK TrailTime Remaining         : 0 days 0 hours
Support Shield State            : Yes
Block SSD Write Disk Cache Change: Yes

                Supported VD Operations
                ================
Read Policy          : Yes
Write Policy         : Yes
IO Policy            : Yes
Access Policy        : Yes
Disk Cache Policy    : Yes
Reconstruction       : Yes
Deny Locate          : No
Deny CC              : No
Allow Ctrl Encryption: No
Enable LDBBM         : No
Support Breakmirror  : No
Power Savings        : No

                Supported PD Operations
                ================
Force Online                            : Yes
Force Offline                           : Yes
Force Rebuild                           : Yes
Deny Force Failed                       : No
Deny Force Good/Bad                     : No
Deny Missing Replace                    : No
Deny Clear                              : No
Deny Locate                             : No
Support Temperature                     : Yes
Disable Copyback                        : No
Enable JBOD                             : No
Enable Copyback on SMART                : Yes
Enable Copyback to SSD on SMART Error   : Yes
Enable SSD Patrol Read                  : No
PR Correct Unconfigured Areas           : No
                Error Counters
                ================
Memory Correctable Errors   : 0 
Memory Uncorrectable Errors : 0 

                High Availability Properties
                ================
Topology Type                 : None
                Cluster Information
                ================
Cluster Permitted     : No
Cluster Active        : No

                Default Settings
                ================
Phy Polarity                     : 0 
Phy PolaritySplit                : 0 
Background Rate                  : 30 
Strip Size                       : 256kB
Flush Time                       : 4 seconds
Write Policy                     : WB
Read Policy                      : Adaptive
Cache When BBU Bad               : Disabled
Cached IO                        : No
SMART Mode                       : Mode 6
Alarm Disable                    : No
Coercion Mode                    : 1GB
ZCR Config                       : Unknown
Dirty LED Shows Drive Activity   : No
BIOS Continue on Error           : 0 
Spin Down Mode                   : None
Allowed Device Type              : SAS/SATA Mix
Allow Mix in Enclosure           : Yes
Allow HDD SAS/SATA Mix in VD     : No
Allow SSD SAS/SATA Mix in VD     : No
Allow HDD/SSD Mix in VD          : No
Allow SATA in Cluster            : No
Max Chained Enclosures           : 16 
Disable Ctrl-R                   : Yes
Enable Web BIOS                  : No
Direct PD Mapping                : No
BIOS Enumerate VDs               : Yes
Restore Hot Spare on Insertion   : No
Expose Enclosure Devices         : Yes
Maintain PD Fail History         : Yes
Disable Puncturing               : Yes
Zero Based Enclosure Enumeration : No
PreBoot CLI Enabled              : No
LED Show Drive Activity          : Yes
Cluster Disable                  : Yes
SAS Disable                      : No
Auto Detect BackPlane Enable     : SGPIO/i2c SEP
Use FDE Only                     : Yes
Enable Led Header                : No
Delay during POST                : 0 
EnableCrashDump                  : No
Disable Online Controller Reset  : No
EnableLDBBM                      : No
Un-Certified Hard Disk Drives    : Allow
Treat Single span R1E as R10     : No
Max LD per array                 : 64
Power Saving option              : All power saving options are disabled
Default spin down time in minutes: 30 
Enable JBOD                      : No
TTY Log In Flash                 : No
Auto Enhanced Import             : Yes
BreakMirror RAID Support         : No
Disable Join Mirror              : No
Enable Shield State              : Yes
Time taken to detect CME         : 60s

Exit Code: 0x00

                                     
    Number of enclosures on adapter 2 -- 3

    Enclosure 0:
    Device ID                     : 25
    Number of Slots               : 24
    Number of Power Supplies      : 2
    Number of Fans                : 2
    Number of Temperature Sensors : 4
    Number of Alarms              : 0
    Number of SIM Modules         : 2
    Number of Physical Drives     : 9
    Status                        : Normal
    Position                      : 1
    Connector Name                : Port 0 - 3
    Enclosure type                : SES
    FRU Part Number               : N/A
    Enclosure Serial Number       : N/A 
    ESM Serial Number             : N/A 
    Enclosure Zoning Mode         : N/A 
    Partner Device Id             : 65535

    Inquiry data                  :
        Vendor Identification     : Lenovo  
        Product Identification    : E1024           
        Product Revision Level    : 2038
        Vendor Specific           :                     

Number of Voltage Sensors         :10

Voltage Sensor                    :0
Voltage Sensor Status             :OK
Voltage Value                     :11810 milli volts

Voltage Sensor                    :1
Voltage Sensor Status             :OK
Voltage Value                     :5050 milli volts

Voltage Sensor                    :2
Voltage Sensor Status             :Not Installed
Voltage Value                     :0 milli volts

Voltage Sensor                    :3
Voltage Sensor Status             :Not Installed
Voltage Value                     :0 milli volts

Voltage Sensor                    :4
Voltage Sensor Status             :OK
Voltage Value                     :11580 milli volts

Voltage Sensor                    :5
Voltage Sensor Status             :OK
Voltage Value                     :5070 milli volts

Voltage Sensor                    :6
Voltage Sensor Status             :OK
Voltage Value                     :3360 milli volts

Voltage Sensor                    :7
Voltage Sensor Status             :OK
Voltage Value                     :11980 milli volts

Voltage Sensor                    :8
Voltage Sensor Status             :OK
Voltage Value                     :5080 milli volts

Voltage Sensor                    :9
Voltage Sensor Status             :OK
Voltage Value                     :3370 milli volts

Number of Power Supplies     : 2 

Power Supply                 : 0 
Power Supply Status          : OK

Power Supply                 : 1 
Power Supply Status          : OK

Number of Fans               : 2 

Fan                          : 0 
Fan Speed              :Low Speed
Fan Status                   : OK

Fan                          : 1 
Fan Speed              :Low Speed
Fan Status                   : OK

Number of Temperature Sensors : 4 

Temp Sensor                  : 0 
Temperature                  : 53 
Temperature Sensor Status    : OK

Temp Sensor                  : 1 
Temperature                  : 53 
Temperature Sensor Status    : OK

Temp Sensor                  : 2 
Temperature                  : 53 
Temperature Sensor Status    : OK

Temp Sensor                  : 3 
Temperature                  : 53 
Temperature Sensor Status    : OK

Number of Chassis             : 1 

Chassis                      : 0 
Chassis Status               : OK

    Enclosure 1:
    Device ID                     : 26
    Number of Slots               : 24
    Number of Power Supplies      : 2
    Number of Fans                : 2
    Number of Temperature Sensors : 4
    Number of Alarms              : 0
    Number of SIM Modules         : 2
    Number of Physical Drives     : 8
    Status                        : Normal
    Position                      : 1
    Connector Name                : Port 4 - 7
    Enclosure type                : SES
    FRU Part Number               : N/A
    Enclosure Serial Number       : N/A 
    ESM Serial Number             : N/A 
    Enclosure Zoning Mode         : N/A 
    Partner Device Id             : 65535

    Inquiry data                  :
        Vendor Identification     : Lenovo  
        Product Identification    : E1024           
        Product Revision Level    : 2038
        Vendor Specific           :                     

Number of Voltage Sensors         :10

Voltage Sensor                    :0
Voltage Sensor Status             :OK
Voltage Value                     :11810 milli volts

Voltage Sensor                    :1
Voltage Sensor Status             :OK
Voltage Value                     :5030 milli volts

Voltage Sensor                    :2
Voltage Sensor Status             :Not Installed
Voltage Value                     :0 milli volts

Voltage Sensor                    :3
Voltage Sensor Status             :Not Installed
Voltage Value                     :0 milli volts

Voltage Sensor                    :4
Voltage Sensor Status             :OK
Voltage Value                     :11980 milli volts

Voltage Sensor                    :5
Voltage Sensor Status             :OK
Voltage Value                     :5050 milli volts

Voltage Sensor                    :6
Voltage Sensor Status             :OK
Voltage Value                     :3380 milli volts

Voltage Sensor                    :7
Voltage Sensor Status             :OK
Voltage Value                     :11560 milli volts

Voltage Sensor                    :8
Voltage Sensor Status             :OK
Voltage Value                     :5060 milli volts

Voltage Sensor                    :9
Voltage Sensor Status             :OK
Voltage Value                     :3360 milli volts

Number of Power Supplies     : 2 

Power Supply                 : 0 
Power Supply Status          : OK

Power Supply                 : 1 
Power Supply Status          : OK

Number of Fans               : 2 

Fan                          : 0 
Fan Speed              :Low Speed
Fan Status                   : OK

Fan                          : 1 
Fan Speed              :Low Speed
Fan Status                   : OK

Number of Temperature Sensors : 4 

Temp Sensor                  : 0 
Temperature                  : 48 
Temperature Sensor Status    : OK

Temp Sensor                  : 1 
Temperature                  : 48 
Temperature Sensor Status    : OK

Temp Sensor                  : 2 
Temperature                  : 48 
Temperature Sensor Status    : OK

Temp Sensor                  : 3 
Temperature                  : 48 
Temperature Sensor Status    : OK

Number of Chassis             : 1 

Chassis                      : 0 
Chassis Status               : OK

    Enclosure 2:
    Device ID                     : 252
    Number of Slots               : 8
    Number of Power Supplies      : 0
    Number of Fans                : 0
    Number of Temperature Sensors : 0
    Number of Alarms              : 0
    Number of SIM Modules         : 1
    Number of Physical Drives     : 0
    Status                        : Normal
    Position                      : 1
    Connector Name                : Unavailable
    Enclosure type                : SGPIO
    FRU Part Number               : N/A
    Enclosure Serial Number       : N/A 
    ESM Serial Number             : N/A 
    Enclosure Zoning Mode         : N/A 
    Partner Device Id             : Unavailable

    Inquiry data                  :
        Vendor Identification     : LSI     
        Product Identification    : SGPIO           
        Product Revision Level    : N/A 
        Vendor Specific           :                     


Exit Code: 0x00

                                     

Adapter 2 -- Virtual Drive Information:
Virtual Drive: 0 (Target Id: 0)
Name                :Data4
RAID Level          : Primary-5, Secondary-0, RAID Level Qualifier-3
Size                : 11.626 TB
Is VD emulated      : Yes
Parity Size         : 744.125 GB
State               : Optimal
Strip Size          : 64 KB
Number Of Drives    : 17
Span Depth          : 1
Default Cache Policy: WriteThrough, ReadAheadNone, Direct, No Write Cache if Bad BBU
Current Cache Policy: WriteThrough, ReadAheadNone, Direct, No Write Cache if Bad BBU
Default Access Policy: Read/Write
Current Access Policy: Read/Write
Disk Cache Policy   : Disk's Default
Encryption Type     : None
PI type: No PI

Is VD Cached: No



Exit Code: 0x00

                                     
Activated Advanced Software Options
---------------------------

Advanced Software Option          : MegaRAID FastPath
Time Remaining   : Unlimited

Advanced Software Option          : MegaRAID RAID5
Time Remaining   : Unlimited


Re-host Information 
--------------------

Needs Re-hosting : No

Exit Code: 0x00
