Level	Date and Time	Source	Event ID	Task Category
Information	12/9/2015 3:37:39 PM	Service Control Manager	7036	None	The Software Protection service entered the running state.
Information	12/9/2015 3:37:39 PM	Service Control Manager	7036	None	The Distributed Transaction Coordinator service entered the running state.
Information	12/9/2015 3:37:38 PM	Service Control Manager	7036	None	The Diagnostic Policy Service service entered the running state.
Information	12/9/2015 3:36:26 PM	Microsoft-Windows-Kernel-General	1	None	"The system time has changed to ‎2015‎-‎12‎-‎09T20:36:26.250000000Z from ‎2015‎-‎12‎-‎09T20:36:26.217346300Z.

Change Reason: An application or system component changed the time."
Information	12/9/2015 3:36:19 PM	Service Control Manager	7036	None	The Software Protection service entered the stopped state.
Information	12/9/2015 3:35:53 PM	Microsoft-Windows-TPM-WMI	1026	None	"The Trusted Platform Module (TPM) hardware on this computer cannot be provisioned for use automatically.  To set up the TPM interactively use the TPM management console (Start->tpm.msc) and use the action to make the TPM ready.

Error: The TPM provisioning action is not allowed by the specified flags.  For provisioning to be successful, one of several actions may be required.  The TPM management console (tpm.msc) action to make the TPM Ready may help.  For further information, see the documentation for the Win32_Tpm WMI method 'Provision'.  (The actions that may be required include importing the TPM Owner Authorization value into the system, calling the Win32_Tpm WMI method for provisioning the TPM and specifying TRUE for either 'ForceClear_Allowed' or 'PhysicalPresencePrompts_Allowed' (as indicated by the value returned in the Additional Information), or enabling the TPM in the system BIOS.)
Additional Information: RebootRequired,TpmForceClearOrImportOwnerAuthRequired,TpmPhysicalPresenceRequired,TpmDelegationSync"
Information	12/9/2015 3:35:53 PM	Microsoft-Windows-TPM-WMI	1282	None	The TBS device identifier has been generated.
Information	12/9/2015 3:35:51 PM	Microsoft-Windows-TPM-WMI	1026	None	"The Trusted Platform Module (TPM) hardware on this computer cannot be provisioned for use automatically.  To set up the TPM interactively use the TPM management console (Start->tpm.msc) and use the action to make the TPM ready.

Error: The TPM provisioning action is not allowed by the specified flags.  For provisioning to be successful, one of several actions may be required.  The TPM management console (tpm.msc) action to make the TPM Ready may help.  For further information, see the documentation for the Win32_Tpm WMI method 'Provision'.  (The actions that may be required include importing the TPM Owner Authorization value into the system, calling the Win32_Tpm WMI method for provisioning the TPM and specifying TRUE for either 'ForceClear_Allowed' or 'PhysicalPresencePrompts_Allowed' (as indicated by the value returned in the Additional Information), or enabling the TPM in the system BIOS.)
Additional Information: RebootRequired,TpmForceClearOrImportOwnerAuthRequired,TpmPhysicalPresenceRequired,TpmDelegationSync"
Information	12/9/2015 3:35:51 PM	Microsoft-Windows-TPM-WMI	1282	None	The TBS device identifier has been generated.
Information	12/9/2015 3:35:47 PM	Service Control Manager	7036	None	The Software Protection service entered the running state.
Information	12/9/2015 3:35:41 PM	Microsoft-Windows-Winlogon	7001	(1101)	User Logon Notification for Customer Experience Improvement Program
Information	12/9/2015 3:35:41 PM	Service Control Manager	7036	None	The Remote Desktop Services UserMode Port Redirector service entered the running state.
Information	12/9/2015 3:35:40 PM	Service Control Manager	7036	None	The Windows Update service entered the running state.
Information	12/9/2015 3:35:40 PM	Service Control Manager	7036	None	The Network Connectivity Assistant service entered the stopped state.
Information	12/9/2015 3:35:40 PM	Service Control Manager	7036	None	The Remote Desktop Configuration service entered the running state.
Information	12/9/2015 3:35:40 PM	Service Control Manager	7036	None	The Certificate Propagation service entered the running state.
Information	12/9/2015 3:35:39 PM	Microsoft-Windows-Iphlpsvc	4200	None	Isatap interface isatap.{74ECDC34-FEDB-4D7B-A2C0-8F6CA5C1F90D} with address fe80::5efe:10.30.1.1 has been brought up.
Information	12/9/2015 3:35:39 PM	Microsoft-Windows-Iphlpsvc	4200	None	Isatap interface isatap.{A6C590D0-16CF-4B2E-9141-217BED1005D9} with address fe80::5efe:169.254.96.120 has been brought up.
Information	12/9/2015 3:35:39 PM	Microsoft-Windows-Iphlpsvc	4200	None	Isatap interface isatap.{2A46F764-8F4A-442B-9D10-52AC161CC193} with address fe80::5efe:169.254.95.120 has been brought up.
Information	12/9/2015 3:35:39 PM	Microsoft-Windows-Iphlpsvc	4200	None	Isatap interface isatap.{A1D185E8-F52D-4F8F-B683-5DDC4087ED28} with address fe80::5efe:172.19.40.138 has been brought up.
Information	12/9/2015 3:35:39 PM	Microsoft-Windows-Iphlpsvc	4200	None	Isatap interface isatap.{6B2B8E43-687D-42C6-854D-7B305CE71E12} with address fe80::5efe:10.40.1.1 has been brought up.
Information	12/9/2015 3:35:39 PM	Microsoft-Windows-Iphlpsvc	4200	None	Isatap interface isatap.{DEA808B0-9EDD-4204-B4ED-4693C3B510A2} with address fe80::5efe:10.20.1.1 has been brought up.
Information	12/9/2015 3:35:39 PM	Microsoft-Windows-Iphlpsvc	4200	None	Isatap interface isatap.{F04F1C91-6BF4-4769-A4BC-A76C341416AC} with address fe80::5efe:10.10.1.1 has been brought up.
Information	12/9/2015 3:35:39 PM	Service Control Manager	7036	None	The Device Setup Manager service entered the running state.
Information	12/9/2015 3:35:39 PM	Service Control Manager	7036	None	The IPsec Policy Agent service entered the running state.
Information	12/9/2015 3:35:38 PM	Service Control Manager	7036	None	The Remote Desktop Services service entered the running state.
Information	12/9/2015 3:35:38 PM	Service Control Manager	7036	None	The Network List Service service entered the running state.
Information	12/9/2015 3:35:38 PM	Service Control Manager	7036	None	The Portable Device Enumerator Service service entered the running state.
Information	12/9/2015 3:35:38 PM	Service Control Manager	7026	None	"The following boot-start or system-start driver(s) did not load: 
cdrom"
Information	12/9/2015 3:35:38 PM	Service Control Manager	7036	None	The Server service entered the running state.
Information	12/9/2015 3:35:38 PM	Service Control Manager	7036	None	The Windows Remote Management (WS-Management) service entered the running state.
Information	12/9/2015 3:35:38 PM	Service Control Manager	7036	None	The IP Helper service entered the running state.
Information	12/9/2015 3:35:38 PM	Microsoft-Windows-WinRM	10148	None	"The WinRM service is listening for WS-Management requests. 

 User Action 
 Use the following command to see the specific IPs on which WinRM is listening: 

 winrm enumerate winrm/config/listener"
Information	12/9/2015 3:35:38 PM	Service Control Manager	7036	None	The Windows Management Instrumentation service entered the running state.
Information	12/9/2015 3:35:37 PM	Service Control Manager	7036	None	The SQL Server VSS Writer service entered the running state.
Information	12/9/2015 3:35:37 PM	Service Control Manager	7036	None	The Distributed Link Tracking Client service entered the running state.
Information	12/9/2015 3:35:37 PM	Service Control Manager	7036	None	The WinHTTP Web Proxy Auto-Discovery Service service entered the running state.
Information	12/9/2015 3:35:37 PM	Service Control Manager	7036	None	The Network Location Awareness service entered the running state.
Information	12/9/2015 3:35:37 PM	Service Control Manager	7036	None	The Remote Registry service entered the running state.
Information	12/9/2015 3:35:37 PM	Service Control Manager	7036	None	The Cryptographic Services service entered the running state.
Information	12/9/2015 3:35:37 PM	Service Control Manager	7036	None	The IKE and AuthIP IPsec Keying Modules service entered the running state.
Information	12/9/2015 3:35:36 PM	Service Control Manager	7036	None	The Print Spooler service entered the running state.
Information	12/9/2015 3:35:36 PM	Service Control Manager	7036	None	The Security Accounts Manager service entered the running state.
Information	12/9/2015 3:35:36 PM	Service Control Manager	7036	None	The Workstation service entered the running state.
Information	12/9/2015 3:35:36 PM	Service Control Manager	7036	None	The Windows Firewall service entered the running state.
Information	12/9/2015 3:35:36 PM	Service Control Manager	7036	None	The Base Filtering Engine service entered the running state.
Information	12/9/2015 3:35:35 PM	Service Control Manager	7036	None	The Windows Font Cache Service service entered the running state.
Information	12/9/2015 3:35:35 PM	Service Control Manager	7036	None	The Task Scheduler service entered the running state.
Information	12/9/2015 3:35:35 PM	Service Control Manager	7036	None	The Shell Hardware Detection service entered the running state.
Information	12/9/2015 3:35:35 PM	Service Control Manager	7036	None	The DHCP Client service entered the running state.
Information	12/9/2015 3:35:35 PM	Microsoft-Windows-DHCPv6-Client	51046	Service State Event	DHCPv6 client service is started
Information	12/9/2015 3:35:35 PM	Microsoft-Windows-Dhcp-Client	50036	Service State Event	DHCPv4 client service is started
Information	12/9/2015 3:35:35 PM	Service Control Manager	7036	None	The DNS Client service entered the running state.
Information	12/9/2015 3:35:35 PM	Service Control Manager	7036	None	The TCP/IP NetBIOS Helper service entered the running state.
Information	12/9/2015 3:35:35 PM	Service Control Manager	7036	None	The Windows Connection Manager service entered the running state.
Information	12/9/2015 3:35:35 PM	Service Control Manager	7036	None	The Network Store Interface Service service entered the running state.
Information	12/9/2015 3:35:34 PM	Service Control Manager	7036	None	The System Event Notification Service service entered the running state.
Information	12/9/2015 3:35:34 PM	Service Control Manager	7036	None	The Group Policy Client service entered the running state.
Information	12/9/2015 3:35:34 PM	Service Control Manager	7036	None	The User Profile Service service entered the running state.
Information	12/9/2015 3:35:34 PM	Service Control Manager	7036	None	The COM+ Event System service entered the running state.
Information	12/9/2015 3:35:34 PM	Service Control Manager	7036	None	The Themes service entered the running state.
Information	12/9/2015 3:35:34 PM	Service Control Manager	7036	None	The Windows Event Log service entered the running state.
Information	12/9/2015 3:35:33 PM	Microsoft-Windows-FilterManager	6	None	File System Filter 'luafv' (6.3, ‎2014‎-‎02‎-‎22T07:14:25.000000000Z) has successfully loaded and registered with Filter Manager.
Information	12/9/2015 3:35:33 PM	Service Control Manager	7036	None	The System Events Broker service entered the running state.
Information	12/9/2015 3:35:32 PM	Service Control Manager	7036	None	The Local Session Manager service entered the running state.
Information	12/9/2015 3:35:32 PM	Service Control Manager	7036	None	The Background Tasks Infrastructure Service service entered the running state.
Information	12/9/2015 3:35:32 PM	Service Control Manager	7036	None	The Remote Procedure Call (RPC) service entered the running state.
Information	12/9/2015 3:35:32 PM	Service Control Manager	7036	None	The RPC Endpoint Mapper service entered the running state.
Information	12/9/2015 3:35:32 PM	Service Control Manager	7036	None	The DCOM Server Process Launcher service entered the running state.
Information	12/9/2015 3:35:32 PM	Service Control Manager	7036	None	The Power service entered the running state.
Information	12/9/2015 3:35:32 PM	Service Control Manager	7036	None	The Plug and Play service entered the running state.
Information	12/9/2015 3:35:25 PM	Microsoft-Windows-Ntfs	98	None	Volume \\?\Volume{e4307b5e-0e02-4bc0-b840-7cc37d646a45} (\Device\HarddiskVolume38) is healthy.  No action is needed.
Information	12/9/2015 3:35:24 PM	Microsoft-Windows-Ntfs	98	None	Volume \\?\Volume{163c6e9e-4d15-4c40-afe7-510de9aa93bb} (\Device\HarddiskVolume36) is healthy.  No action is needed.
Information	12/9/2015 3:35:23 PM	Microsoft-Windows-Ntfs	98	None	Volume \\?\Volume{5748de44-1cd9-481c-92a4-82305981aa8b} (\Device\HarddiskVolume59) is healthy.  No action is needed.
Information	12/9/2015 3:35:23 PM	Microsoft-Windows-Ntfs	98	None	Volume \\?\Volume{330d458a-c1fd-4aff-bdde-9dc66286897b} (\Device\HarddiskVolume69) is healthy.  No action is needed.
Information	12/9/2015 3:35:22 PM	Microsoft-Windows-Ntfs	98	None	Volume \\?\Volume{b98bf919-32e7-43e1-849e-eaaced39850a} (\Device\HarddiskVolume75) is healthy.  No action is needed.
Information	12/9/2015 3:35:21 PM	Microsoft-Windows-Ntfs	98	None	Volume \\?\Volume{e31ba883-6b02-485e-8383-df3f586c6168} (\Device\HarddiskVolume47) is healthy.  No action is needed.
Information	12/9/2015 3:35:20 PM	Microsoft-Windows-Ntfs	98	None	Volume \\?\Volume{2435955d-0c47-4c96-8239-0caaac83182e} (\Device\HarddiskVolume1) is healthy.  No action is needed.
Information	12/9/2015 3:35:20 PM	Microsoft-Windows-Ntfs	98	None	Volume \\?\Volume{84a8b705-0c34-460d-8581-13f654ccb9fa} (\Device\HarddiskVolume42) is healthy.  No action is needed.
Information	12/9/2015 3:35:19 PM	Microsoft-Windows-Ntfs	98	None	Volume \\?\Volume{4c902526-bdee-4e6a-b928-f10af309271d} (\Device\HarddiskVolume46) is healthy.  No action is needed.
Information	12/9/2015 3:35:18 PM	Microsoft-Windows-Ntfs	98	None	Volume \\?\Volume{ead256c4-e66f-48a9-9021-60cc37712f4d} (\Device\HarddiskVolume33) is healthy.  No action is needed.
Information	12/9/2015 3:35:18 PM	Microsoft-Windows-Ntfs	98	None	Volume \\?\Volume{17458964-9ee2-4732-a1e8-102a03381ca0} (\Device\HarddiskVolume67) is healthy.  No action is needed.
Information	12/9/2015 3:35:18 PM	Microsoft-Windows-Ntfs	98	None	Volume \\?\Volume{8f71ce79-bf4d-4cf5-9912-51e0b7ceba89} (\Device\HarddiskVolume39) is healthy.  No action is needed.
Information	12/9/2015 3:35:17 PM	Microsoft-Windows-Ntfs	98	None	Volume \\?\Volume{0d07cc6f-1601-4180-b5d7-649c8e3fec74} (\Device\HarddiskVolume79) is healthy.  No action is needed.
Information	12/9/2015 3:35:16 PM	Microsoft-Windows-Ntfs	98	None	Volume \\?\Volume{df2fbf69-b023-4ec3-a0fe-0310ca5484c6} (\Device\HarddiskVolume87) is healthy.  No action is needed.
Information	12/9/2015 3:35:16 PM	Microsoft-Windows-Ntfs	98	None	Volume \\?\Volume{593d710b-5728-45c9-a61a-e8f3de26eae2} (\Device\HarddiskVolume49) is healthy.  No action is needed.
Information	12/9/2015 3:35:15 PM	Microsoft-Windows-Ntfs	98	None	Volume \\?\Volume{729b2d84-1193-4625-9c24-c482044db076} (\Device\HarddiskVolume51) is healthy.  No action is needed.
Information	12/9/2015 3:35:15 PM	Microsoft-Windows-Ntfs	98	None	Volume \\?\Volume{d0e055e5-4567-4371-9e67-7184f8d609b0} (\Device\HarddiskVolume35) is healthy.  No action is needed.
Information	12/9/2015 3:35:14 PM	Microsoft-Windows-Ntfs	98	None	Volume \\?\Volume{7f056d30-b74c-4771-9f3b-feeba85c6786} (\Device\HarddiskVolume71) is healthy.  No action is needed.
Information	12/9/2015 3:35:12 PM	Microsoft-Windows-Ntfs	98	None	Volume \\?\Volume{2417d2ce-e5f0-4ccb-9952-0cdc2b905086} (\Device\HarddiskVolume73) is healthy.  No action is needed.
Information	12/9/2015 3:34:42 PM	Microsoft-Windows-Ntfs	98	None	Volume \\?\Volume{6798d74d-ce99-4746-8658-554efe2bb4d0} (\Device\HarddiskVolume41) is healthy.  No action is needed.
Information	12/9/2015 3:34:04 PM	Microsoft-Windows-Ntfs	98	None	Volume \\?\Volume{454715f7-3957-4358-98d5-0150b6f9c15d} (\Device\HarddiskVolume31) is healthy.  No action is needed.
Information	12/9/2015 3:33:52 PM	Microsoft-Windows-Ntfs	98	None	Volume \\?\Volume{456966bd-729e-4b43-bc2e-2f06682bb655} (\Device\HarddiskVolume77) is healthy.  No action is needed.
Information	12/9/2015 3:33:12 PM	Microsoft-Windows-Ntfs	98	None	Volume F: (\Device\HarddiskVolume7) is healthy.  No action is needed.
Information	12/9/2015 3:33:11 PM	Microsoft-Windows-Ntfs	98	None	Volume \\?\Volume{2e52d4ad-cb52-4f6d-b088-e899e97a6533} (\Device\HarddiskVolume44) is healthy.  No action is needed.
Information	12/9/2015 3:32:43 PM	Microsoft-Windows-Ntfs	98	None	Volume T: (\Device\HarddiskVolume89) is healthy.  No action is needed.
Information	12/9/2015 3:32:39 PM	Microsoft-Windows-Ntfs	98	None	Volume \\?\Volume{a4e5ff01-af34-4c7e-98c3-7c75de722f81} (\Device\HarddiskVolume15) is healthy.  No action is needed.
Information	12/9/2015 3:32:32 PM	Microsoft-Windows-Ntfs	98	None	Volume \\?\Volume{1f87331b-f3be-4bb1-a4b3-fda1fc37fadf} (\Device\HarddiskVolume23) is healthy.  No action is needed.
Information	12/9/2015 3:32:06 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 35 in group 7 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:32:06 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 33 in group 7 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:32:06 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 31 in group 7 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:32:06 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 29 in group 7 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:32:06 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 27 in group 7 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:32:05 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 25 in group 7 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:32:05 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 23 in group 7 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:32:05 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 21 in group 7 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:32:05 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 19 in group 7 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:32:05 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 17 in group 7 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:32:05 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 15 in group 7 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:32:04 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 13 in group 7 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:32:04 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 11 in group 7 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:32:04 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 9 in group 7 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:32:04 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 7 in group 7 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:32:04 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 5 in group 7 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:32:04 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 3 in group 7 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:32:04 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 1 in group 7 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:32:04 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 34 in group 7 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:32:04 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 32 in group 7 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:32:03 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 30 in group 7 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:32:03 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 28 in group 7 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:32:03 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 26 in group 7 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:32:03 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 24 in group 7 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:32:03 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 22 in group 7 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:32:03 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 20 in group 7 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:32:03 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 18 in group 7 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:32:03 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 16 in group 7 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:32:03 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 14 in group 7 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:32:03 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 12 in group 7 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:32:03 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 10 in group 7 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:32:02 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 8 in group 7 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:32:02 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 6 in group 7 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:32:02 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 4 in group 7 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:32:02 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 2 in group 7 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:32:02 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 0 in group 7 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:32:02 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 35 in group 6 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:32:02 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 33 in group 6 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:32:02 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 31 in group 6 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:32:02 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 29 in group 6 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:32:01 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 27 in group 6 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:32:01 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 25 in group 6 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:32:01 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 23 in group 6 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:32:01 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 21 in group 6 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:32:01 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 19 in group 6 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:32:01 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 17 in group 6 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:32:01 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 15 in group 6 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:32:01 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 13 in group 6 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:32:01 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 11 in group 6 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:32:00 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 9 in group 6 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:32:00 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 7 in group 6 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:32:00 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 5 in group 6 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:32:00 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 3 in group 6 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:32:00 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 1 in group 6 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:32:00 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 34 in group 6 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:32:00 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 32 in group 6 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:32:00 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 30 in group 6 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:32:00 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 28 in group 6 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:59 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 26 in group 6 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:59 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 24 in group 6 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:59 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 22 in group 6 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:59 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 20 in group 6 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:59 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 18 in group 6 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:59 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 16 in group 6 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:59 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 14 in group 6 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:59 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 12 in group 6 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:59 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 10 in group 6 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:59 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 8 in group 6 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:58 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 6 in group 6 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:58 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 4 in group 6 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:58 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 2 in group 6 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:58 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 0 in group 6 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:58 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 35 in group 5 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:58 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 33 in group 5 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:58 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 31 in group 5 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:58 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 29 in group 5 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:58 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 27 in group 5 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:58 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 25 in group 5 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:57 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 23 in group 5 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:57 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 21 in group 5 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:57 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 19 in group 5 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:57 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 17 in group 5 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:57 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 15 in group 5 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:57 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 13 in group 5 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:56 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 11 in group 5 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:56 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 9 in group 5 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:56 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 7 in group 5 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:56 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 5 in group 5 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:56 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 3 in group 5 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:56 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 1 in group 5 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:56 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 34 in group 5 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:56 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 32 in group 5 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:56 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 30 in group 5 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:56 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 28 in group 5 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:55 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 26 in group 5 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:55 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 24 in group 5 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:55 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 22 in group 5 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:55 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 20 in group 5 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:55 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 18 in group 5 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:55 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 16 in group 5 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:55 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 14 in group 5 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:55 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 12 in group 5 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:55 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 10 in group 5 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:55 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 8 in group 5 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:54 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 6 in group 5 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:54 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 4 in group 5 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:54 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 2 in group 5 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:54 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 0 in group 5 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:54 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 35 in group 4 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:54 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 33 in group 4 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:54 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 31 in group 4 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:54 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 29 in group 4 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:54 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 27 in group 4 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:53 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 25 in group 4 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:53 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 23 in group 4 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:53 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 21 in group 4 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:53 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 19 in group 4 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:53 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 17 in group 4 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:53 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 15 in group 4 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:53 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 13 in group 4 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:53 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 11 in group 4 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:53 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 9 in group 4 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:52 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 7 in group 4 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:52 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 5 in group 4 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:52 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 3 in group 4 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:52 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 1 in group 4 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:52 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 34 in group 4 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:52 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 32 in group 4 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:52 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 30 in group 4 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:52 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 28 in group 4 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:52 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 26 in group 4 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:52 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 24 in group 4 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:51 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 22 in group 4 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:51 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 20 in group 4 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:51 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 18 in group 4 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:51 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 16 in group 4 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:51 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 14 in group 4 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:51 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 12 in group 4 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:51 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 10 in group 4 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:51 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 8 in group 4 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:51 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 6 in group 4 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:51 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 4 in group 4 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:50 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 2 in group 4 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:50 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 0 in group 4 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:50 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 35 in group 3 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:50 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 33 in group 3 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:50 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 31 in group 3 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:50 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 29 in group 3 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:50 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 27 in group 3 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:50 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 25 in group 3 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:50 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 23 in group 3 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:49 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 21 in group 3 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:49 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 19 in group 3 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:49 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 17 in group 3 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:49 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 15 in group 3 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:49 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 13 in group 3 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:49 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 11 in group 3 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:49 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 9 in group 3 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:49 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 7 in group 3 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:49 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 5 in group 3 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:48 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 3 in group 3 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:48 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 1 in group 3 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:48 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 34 in group 3 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:48 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 32 in group 3 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:48 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 30 in group 3 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:48 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 28 in group 3 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:48 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 26 in group 3 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:48 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 24 in group 3 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:48 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 22 in group 3 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:48 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 20 in group 3 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:48 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 18 in group 3 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:47 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 16 in group 3 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:47 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 14 in group 3 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:47 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 12 in group 3 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:47 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 10 in group 3 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:47 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 8 in group 3 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:47 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 6 in group 3 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:47 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 4 in group 3 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:47 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 2 in group 3 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:47 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 0 in group 3 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:47 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 35 in group 2 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:46 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 33 in group 2 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:46 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 31 in group 2 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:46 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 29 in group 2 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:46 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 27 in group 2 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:46 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 25 in group 2 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:46 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 23 in group 2 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:46 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 21 in group 2 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:46 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 19 in group 2 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:46 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 17 in group 2 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:46 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 15 in group 2 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:45 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 13 in group 2 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:45 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 11 in group 2 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:45 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 9 in group 2 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:45 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 7 in group 2 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:45 PM	ixgbt	31	None	"Intel(R) Ethernet Converged Network Ad... [161,0,1]
 Network link has been established at 10Gbps full duplex.
"
Information	12/9/2015 3:31:45 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 5 in group 2 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:45 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 3 in group 2 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:45 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 1 in group 2 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:45 PM	ixgbt	31	None	"Intel(R) Ethernet Converged Network Ad... [225,0,1]
 Network link has been established at 10Gbps full duplex.
"
Information	12/9/2015 3:31:45 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 34 in group 2 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:45 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 32 in group 2 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:44 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 30 in group 2 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:44 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 28 in group 2 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:44 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 26 in group 2 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:44 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 24 in group 2 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:44 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 22 in group 2 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:44 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 20 in group 2 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:44 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 18 in group 2 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:44 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 16 in group 2 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:44 PM	ixgbt	31	None	"Intel(R) Ethernet Converged Network Ada... [65,0,1]
 Network link has been established at 10Gbps full duplex.
"
Information	12/9/2015 3:31:44 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 14 in group 2 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:44 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 12 in group 2 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:44 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 10 in group 2 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:43 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 8 in group 2 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:43 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 6 in group 2 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:43 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 4 in group 2 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:43 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 2 in group 2 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:43 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 0 in group 2 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:43 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 35 in group 1 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:43 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 33 in group 1 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:43 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 31 in group 1 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:43 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 29 in group 1 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:43 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 27 in group 1 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:42 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 25 in group 1 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:42 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 23 in group 1 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:42 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 21 in group 1 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:42 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 19 in group 1 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:42 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 17 in group 1 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:42 PM	ixgbt	31	None	"Intel(R) Ethernet Controller X540-AT2 #3
 Network link has been established at 10Gbps full duplex.
"
Information	12/9/2015 3:31:42 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 15 in group 1 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:42 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 13 in group 1 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:42 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 11 in group 1 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:41 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 9 in group 1 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:41 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 7 in group 1 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:41 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 5 in group 1 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:41 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 3 in group 1 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:41 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 1 in group 1 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Warning	12/9/2015 3:31:41 PM	ixgbt	27	None	"Intel(R) Ethernet Converged Network Ad... [161,0,1]
 Network link is disconnected.
"
Information	12/9/2015 3:31:41 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 34 in group 1 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:41 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 32 in group 1 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:41 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 30 in group 1 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:41 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 28 in group 1 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Warning	12/9/2015 3:31:41 PM	ixgbt	27	None	"Intel(R) Ethernet Converged Network Ad... [225,0,1]
 Network link is disconnected.
"
Information	12/9/2015 3:31:41 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 26 in group 1 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:41 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 24 in group 1 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:40 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 22 in group 1 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:40 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 20 in group 1 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:40 PM	ixgbt	32	None	"Intel(R) Ethernet Controller X540-AT2 #4
 Network link has been established at 1Gbps full duplex.
"
Information	12/9/2015 3:31:40 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 18 in group 1 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:40 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 16 in group 1 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:40 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 14 in group 1 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:40 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 12 in group 1 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:40 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 10 in group 1 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:40 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 8 in group 1 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:40 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 6 in group 1 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Warning	12/9/2015 3:31:40 PM	ixgbt	27	None	"Intel(R) Ethernet Converged Network Ada... [65,0,1]
 Network link is disconnected.
"
Information	12/9/2015 3:31:40 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 4 in group 1 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:40 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 2 in group 1 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:39 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 0 in group 1 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:39 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 35 in group 0 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:39 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 33 in group 0 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:39 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 31 in group 0 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:39 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 29 in group 0 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:39 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 27 in group 0 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:39 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 25 in group 0 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:39 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 23 in group 0 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:39 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 21 in group 0 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:38 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 19 in group 0 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:38 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 17 in group 0 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:38 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 15 in group 0 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Warning	12/9/2015 3:31:38 PM	ixgbt	27	None	"Intel(R) Ethernet Controller X540-AT2 #4
 Network link is disconnected.
"
Information	12/9/2015 3:31:38 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 13 in group 0 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:38 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 11 in group 0 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:38 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 9 in group 0 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Warning	12/9/2015 3:31:38 PM	ixgbt	27	None	"Intel(R) Ethernet Controller X540-AT2 #3
 Network link is disconnected.
"
Information	12/9/2015 3:31:38 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 7 in group 0 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:38 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 5 in group 0 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:38 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 3 in group 0 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:38 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 1 in group 0 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:37 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 34 in group 0 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:37 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 32 in group 0 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:37 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 30 in group 0 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:37 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 28 in group 0 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:37 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 26 in group 0 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:37 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 24 in group 0 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:37 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 22 in group 0 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:37 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 20 in group 0 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:37 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 18 in group 0 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:37 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 16 in group 0 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:37 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 14 in group 0 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:36 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 12 in group 0 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:36 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 10 in group 0 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:36 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 8 in group 0 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:36 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 6 in group 0 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:36 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 4 in group 0 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:36 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 2 in group 0 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 3:31:36 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 0 in group 0 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Critical	12/9/2015 3:30:54 PM	Microsoft-Windows-Kernel-Power	41	(63)	The system has rebooted without cleanly shutting down first. This error could be caused if the system stopped responding, crashed, or lost power unexpectedly.
Information	12/9/2015 3:30:52 PM	Microsoft-Windows-FilterManager	6	None	File System Filter 'npsvctrig' (6.3, ‎2013‎-‎08‎-‎22T06:38:22.000000000Z) has successfully loaded and registered with Filter Manager.
Information	12/9/2015 3:30:01 PM	Microsoft-Windows-Ntfs	98	None	Volume C: (\Device\HarddiskVolume4) is healthy.  No action is needed.
Information	12/9/2015 3:28:33 PM	TPM	24	None	The Trusted Platform Module (TPM) status: Enabled and Active.
Information	12/9/2015 3:35:34 PM	EventLog	6013	None	The system uptime is 606 seconds.
Information	12/9/2015 3:35:34 PM	EventLog	6005	None	The Event log service was started.
Information	12/9/2015 3:35:34 PM	EventLog	6009	None	Microsoft (R) Windows (R) 6.03. 9600  Multiprocessor Free.
Error	12/9/2015 3:35:34 PM	EventLog	6008	None	The previous system shutdown at 2:58:49 PM on ‎12/‎9/‎2015 was unexpected.
Information	12/9/2015 3:27:07 PM	Microsoft-Windows-Kernel-Boot	27	None	The boot type was 0x0.
Information	12/9/2015 3:27:07 PM	Microsoft-Windows-Kernel-Boot	20	None	The last shutdown's success status was false. The last boot's success status was true.
Information	12/9/2015 3:27:07 PM	Microsoft-Windows-Kernel-Boot	32	None	The bootmgr spent 0 ms waiting for user input.
Information	12/9/2015 3:27:07 PM	Microsoft-Windows-Kernel-Boot	18	None	There are 0x1 boot options on this system.
Information	12/9/2015 3:27:07 PM	Microsoft-Windows-Kernel-General	12	None	The operating system started at system time ‎2015‎-‎12‎-‎09T20:25:27.490342600Z.
Information	12/9/2015 2:23:46 PM	Service Control Manager	7045	None	"A service was installed in the system.

Service Name:  WinRing0_1_2_0
Service File Name:  C:\Tools\CPUSpeed\WinRing0x64.sys
Service Type:  kernel mode driver
Service Start Type:  demand start
Service Account:  "
Information	12/9/2015 2:11:21 PM	Service Control Manager	7036	None	The WinHTTP Web Proxy Auto-Discovery Service service entered the stopped state.
Information	12/9/2015 1:52:55 PM	Service Control Manager	7036	None	The Windows Update service entered the stopped state.
Information	12/9/2015 1:52:51 PM	Service Control Manager	7036	None	The Remote Registry service entered the stopped state.
Information	12/9/2015 1:51:52 PM	Service Control Manager	7045	None	"A service was installed in the system.

Service Name:  WinRing0_1_2_0
Service File Name:  C:\Tools\CPUSpeed\WinRing0x64.sys
Service Type:  kernel mode driver
Service Start Type:  demand start
Service Account:  "
Information	12/9/2015 1:45:23 PM	Service Control Manager	7036	None	The Software Protection service entered the stopped state.
Information	12/9/2015 1:45:03 PM	Service Control Manager	7036	None	The User Access Logging Service service entered the running state.
Information	12/9/2015 1:44:53 PM	Service Control Manager	7036	None	The Software Protection service entered the running state.
Information	12/9/2015 1:44:53 PM	Service Control Manager	7036	None	The Distributed Transaction Coordinator service entered the running state.
Information	12/9/2015 1:44:53 PM	Service Control Manager	7036	None	The Portable Device Enumerator Service service entered the stopped state.
Information	12/9/2015 1:44:52 PM	Service Control Manager	7036	None	The Diagnostic Policy Service service entered the running state.
Information	12/9/2015 1:43:37 PM	Microsoft-Windows-Kernel-General	1	None	"The system time has changed to ‎2015‎-‎12‎-‎09T18:43:37.490000000Z from ‎2015‎-‎12‎-‎09T18:43:38.062328000Z.

Change Reason: An application or system component changed the time."
Information	12/9/2015 1:43:31 PM	Service Control Manager	7036	None	The Software Protection service entered the stopped state.
Information	12/9/2015 1:43:05 PM	Microsoft-Windows-TPM-WMI	1026	None	"The Trusted Platform Module (TPM) hardware on this computer cannot be provisioned for use automatically.  To set up the TPM interactively use the TPM management console (Start->tpm.msc) and use the action to make the TPM ready.

Error: The TPM provisioning action is not allowed by the specified flags.  For provisioning to be successful, one of several actions may be required.  The TPM management console (tpm.msc) action to make the TPM Ready may help.  For further information, see the documentation for the Win32_Tpm WMI method 'Provision'.  (The actions that may be required include importing the TPM Owner Authorization value into the system, calling the Win32_Tpm WMI method for provisioning the TPM and specifying TRUE for either 'ForceClear_Allowed' or 'PhysicalPresencePrompts_Allowed' (as indicated by the value returned in the Additional Information), or enabling the TPM in the system BIOS.)
Additional Information: RebootRequired,TpmForceClearOrImportOwnerAuthRequired,TpmPhysicalPresenceRequired,TpmDelegationSync"
Information	12/9/2015 1:43:05 PM	Microsoft-Windows-TPM-WMI	1282	None	The TBS device identifier has been generated.
Information	12/9/2015 1:43:03 PM	Microsoft-Windows-TPM-WMI	1026	None	"The Trusted Platform Module (TPM) hardware on this computer cannot be provisioned for use automatically.  To set up the TPM interactively use the TPM management console (Start->tpm.msc) and use the action to make the TPM ready.

Error: The TPM provisioning action is not allowed by the specified flags.  For provisioning to be successful, one of several actions may be required.  The TPM management console (tpm.msc) action to make the TPM Ready may help.  For further information, see the documentation for the Win32_Tpm WMI method 'Provision'.  (The actions that may be required include importing the TPM Owner Authorization value into the system, calling the Win32_Tpm WMI method for provisioning the TPM and specifying TRUE for either 'ForceClear_Allowed' or 'PhysicalPresencePrompts_Allowed' (as indicated by the value returned in the Additional Information), or enabling the TPM in the system BIOS.)
Additional Information: RebootRequired,TpmForceClearOrImportOwnerAuthRequired,TpmPhysicalPresenceRequired,TpmDelegationSync"
Information	12/9/2015 1:43:03 PM	Microsoft-Windows-TPM-WMI	1282	None	The TBS device identifier has been generated.
Information	12/9/2015 1:42:58 PM	Service Control Manager	7036	None	The Software Protection service entered the running state.
Information	12/9/2015 1:42:55 PM	Service Control Manager	7036	None	The Remote Desktop Services UserMode Port Redirector service entered the running state.
Information	12/9/2015 1:42:54 PM	Service Control Manager	7036	None	The Remote Desktop Configuration service entered the running state.
Information	12/9/2015 1:42:54 PM	Service Control Manager	7036	None	The Certificate Propagation service entered the running state.
Information	12/9/2015 1:42:54 PM	Service Control Manager	7036	None	The Windows Update service entered the running state.
Information	12/9/2015 1:42:53 PM	Service Control Manager	7036	None	The IPsec Policy Agent service entered the running state.
Information	12/9/2015 1:42:53 PM	Service Control Manager	7036	None	The Network Connectivity Assistant service entered the stopped state.
Information	12/9/2015 1:42:53 PM	Microsoft-Windows-Iphlpsvc	4200	None	Isatap interface isatap.{74ECDC34-FEDB-4D7B-A2C0-8F6CA5C1F90D} with address fe80::5efe:10.30.1.1 has been brought up.
Information	12/9/2015 1:42:53 PM	Microsoft-Windows-Iphlpsvc	4200	None	Isatap interface isatap.{A6C590D0-16CF-4B2E-9141-217BED1005D9} with address fe80::5efe:169.254.96.120 has been brought up.
Information	12/9/2015 1:42:53 PM	Microsoft-Windows-Iphlpsvc	4200	None	Isatap interface isatap.{2A46F764-8F4A-442B-9D10-52AC161CC193} with address fe80::5efe:169.254.95.120 has been brought up.
Information	12/9/2015 1:42:53 PM	Microsoft-Windows-Iphlpsvc	4200	None	Isatap interface isatap.{A1D185E8-F52D-4F8F-B683-5DDC4087ED28} with address fe80::5efe:172.19.40.138 has been brought up.
Information	12/9/2015 1:42:53 PM	Microsoft-Windows-Iphlpsvc	4200	None	Isatap interface isatap.{6B2B8E43-687D-42C6-854D-7B305CE71E12} with address fe80::5efe:10.40.1.1 has been brought up.
Information	12/9/2015 1:42:53 PM	Microsoft-Windows-Iphlpsvc	4200	None	Isatap interface isatap.{DEA808B0-9EDD-4204-B4ED-4693C3B510A2} with address fe80::5efe:10.20.1.1 has been brought up.
Information	12/9/2015 1:42:53 PM	Service Control Manager	7036	None	The Portable Device Enumerator Service service entered the running state.
Information	12/9/2015 1:42:53 PM	Service Control Manager	7036	None	The Device Setup Manager service entered the running state.
Information	12/9/2015 1:42:53 PM	Microsoft-Windows-Iphlpsvc	4200	None	Isatap interface isatap.{F04F1C91-6BF4-4769-A4BC-A76C341416AC} with address fe80::5efe:10.10.1.1 has been brought up.
Information	12/9/2015 1:42:53 PM	Service Control Manager	7036	None	The Remote Desktop Services service entered the running state.
Information	12/9/2015 1:42:53 PM	Service Control Manager	7036	None	The Network List Service service entered the running state.
Information	12/9/2015 1:42:53 PM	Service Control Manager	7026	None	"The following boot-start or system-start driver(s) did not load: 
cdrom"
Information	12/9/2015 1:42:53 PM	Service Control Manager	7036	None	The Server service entered the running state.
Information	12/9/2015 1:42:52 PM	Service Control Manager	7036	None	The IP Helper service entered the running state.
Information	12/9/2015 1:42:52 PM	Service Control Manager	7036	None	The Windows Remote Management (WS-Management) service entered the running state.
Information	12/9/2015 1:42:52 PM	Service Control Manager	7036	None	The Windows Management Instrumentation service entered the running state.
Information	12/9/2015 1:42:52 PM	Service Control Manager	7036	None	The Distributed Link Tracking Client service entered the running state.
Information	12/9/2015 1:42:52 PM	Service Control Manager	7036	None	The SQL Server VSS Writer service entered the running state.
Information	12/9/2015 1:42:52 PM	Service Control Manager	7036	None	The WinHTTP Web Proxy Auto-Discovery Service service entered the running state.
Information	12/9/2015 1:42:52 PM	Microsoft-Windows-Winlogon	7001	(1101)	User Logon Notification for Customer Experience Improvement Program
Information	12/9/2015 1:42:51 PM	Service Control Manager	7036	None	The Network Location Awareness service entered the running state.
Information	12/9/2015 1:42:51 PM	Service Control Manager	7036	None	The Remote Registry service entered the running state.
Information	12/9/2015 1:42:51 PM	Service Control Manager	7036	None	The IKE and AuthIP IPsec Keying Modules service entered the running state.
Information	12/9/2015 1:42:51 PM	Service Control Manager	7036	None	The Cryptographic Services service entered the running state.
Information	12/9/2015 1:42:52 PM	Microsoft-Windows-WinRM	10148	None	"The WinRM service is listening for WS-Management requests. 

 User Action 
 Use the following command to see the specific IPs on which WinRM is listening: 

 winrm enumerate winrm/config/listener"
Information	12/9/2015 1:42:51 PM	Service Control Manager	7036	None	The Print Spooler service entered the running state.
Information	12/9/2015 1:42:51 PM	Service Control Manager	7036	None	The Security Accounts Manager service entered the running state.
Information	12/9/2015 1:42:51 PM	Service Control Manager	7036	None	The Workstation service entered the running state.
Information	12/9/2015 1:42:50 PM	Service Control Manager	7036	None	The Windows Firewall service entered the running state.
Information	12/9/2015 1:42:50 PM	Service Control Manager	7036	None	The Base Filtering Engine service entered the running state.
Information	12/9/2015 1:42:50 PM	Service Control Manager	7036	None	The Windows Font Cache Service service entered the running state.
Information	12/9/2015 1:42:50 PM	Service Control Manager	7036	None	The Task Scheduler service entered the running state.
Information	12/9/2015 1:42:50 PM	Service Control Manager	7036	None	The Shell Hardware Detection service entered the running state.
Information	12/9/2015 1:42:50 PM	Service Control Manager	7036	None	The DHCP Client service entered the running state.
Information	12/9/2015 1:42:50 PM	Microsoft-Windows-DHCPv6-Client	51046	Service State Event	DHCPv6 client service is started
Information	12/9/2015 1:42:49 PM	Service Control Manager	7036	None	The DNS Client service entered the running state.
Information	12/9/2015 1:42:49 PM	Microsoft-Windows-Dhcp-Client	50036	Service State Event	DHCPv4 client service is started
Information	12/9/2015 1:42:49 PM	Service Control Manager	7036	None	The TCP/IP NetBIOS Helper service entered the running state.
Information	12/9/2015 1:42:49 PM	Service Control Manager	7036	None	The Windows Connection Manager service entered the running state.
Information	12/9/2015 1:42:49 PM	Service Control Manager	7036	None	The Network Store Interface Service service entered the running state.
Information	12/9/2015 1:42:49 PM	Service Control Manager	7036	None	The Group Policy Client service entered the running state.
Information	12/9/2015 1:42:49 PM	Service Control Manager	7036	None	The User Profile Service service entered the running state.
Information	12/9/2015 1:42:49 PM	Service Control Manager	7036	None	The System Event Notification Service service entered the running state.
Information	12/9/2015 1:42:48 PM	Service Control Manager	7036	None	The COM+ Event System service entered the running state.
Information	12/9/2015 1:42:48 PM	Service Control Manager	7036	None	The Themes service entered the running state.
Information	12/9/2015 1:42:48 PM	Service Control Manager	7036	None	The Windows Event Log service entered the running state.
Information	12/9/2015 1:42:48 PM	Microsoft-Windows-FilterManager	6	None	File System Filter 'luafv' (6.3, ‎2014‎-‎02‎-‎22T07:14:25.000000000Z) has successfully loaded and registered with Filter Manager.
Information	12/9/2015 1:42:48 PM	Service Control Manager	7036	None	The System Events Broker service entered the running state.
Information	12/9/2015 1:42:48 PM	Service Control Manager	7036	None	The Local Session Manager service entered the running state.
Information	12/9/2015 1:42:48 PM	Service Control Manager	7036	None	The Background Tasks Infrastructure Service service entered the running state.
Information	12/9/2015 1:42:47 PM	Service Control Manager	7036	None	The Remote Procedure Call (RPC) service entered the running state.
Information	12/9/2015 1:42:47 PM	Service Control Manager	7036	None	The RPC Endpoint Mapper service entered the running state.
Information	12/9/2015 1:42:47 PM	Service Control Manager	7036	None	The DCOM Server Process Launcher service entered the running state.
Information	12/9/2015 1:42:47 PM	Service Control Manager	7036	None	The Power service entered the running state.
Information	12/9/2015 1:42:47 PM	Service Control Manager	7036	None	The Plug and Play service entered the running state.
Information	12/9/2015 1:42:42 PM	Microsoft-Windows-Ntfs	98	None	Volume \\?\Volume{e4307b5e-0e02-4bc0-b840-7cc37d646a45} (\Device\HarddiskVolume38) is healthy.  No action is needed.
Information	12/9/2015 1:42:41 PM	Microsoft-Windows-Ntfs	98	None	Volume \\?\Volume{163c6e9e-4d15-4c40-afe7-510de9aa93bb} (\Device\HarddiskVolume36) is healthy.  No action is needed.
Information	12/9/2015 1:42:40 PM	Microsoft-Windows-Ntfs	98	None	Volume \\?\Volume{5748de44-1cd9-481c-92a4-82305981aa8b} (\Device\HarddiskVolume59) is healthy.  No action is needed.
Information	12/9/2015 1:42:40 PM	Microsoft-Windows-Ntfs	98	None	Volume \\?\Volume{330d458a-c1fd-4aff-bdde-9dc66286897b} (\Device\HarddiskVolume69) is healthy.  No action is needed.
Information	12/9/2015 1:42:39 PM	Microsoft-Windows-Ntfs	98	None	Volume \\?\Volume{b98bf919-32e7-43e1-849e-eaaced39850a} (\Device\HarddiskVolume75) is healthy.  No action is needed.
Information	12/9/2015 1:42:38 PM	Microsoft-Windows-Ntfs	98	None	Volume \\?\Volume{e31ba883-6b02-485e-8383-df3f586c6168} (\Device\HarddiskVolume47) is healthy.  No action is needed.
Information	12/9/2015 1:42:37 PM	Microsoft-Windows-Ntfs	98	None	Volume \\?\Volume{2435955d-0c47-4c96-8239-0caaac83182e} (\Device\HarddiskVolume1) is healthy.  No action is needed.
Information	12/9/2015 1:42:37 PM	Microsoft-Windows-Ntfs	98	None	Volume \\?\Volume{84a8b705-0c34-460d-8581-13f654ccb9fa} (\Device\HarddiskVolume42) is healthy.  No action is needed.
Information	12/9/2015 1:42:36 PM	Microsoft-Windows-Ntfs	98	None	Volume \\?\Volume{4c902526-bdee-4e6a-b928-f10af309271d} (\Device\HarddiskVolume46) is healthy.  No action is needed.
Information	12/9/2015 1:42:35 PM	Microsoft-Windows-Ntfs	98	None	Volume \\?\Volume{ead256c4-e66f-48a9-9021-60cc37712f4d} (\Device\HarddiskVolume33) is healthy.  No action is needed.
Information	12/9/2015 1:42:35 PM	Microsoft-Windows-Ntfs	98	None	Volume \\?\Volume{17458964-9ee2-4732-a1e8-102a03381ca0} (\Device\HarddiskVolume67) is healthy.  No action is needed.
Information	12/9/2015 1:42:34 PM	Microsoft-Windows-Ntfs	98	None	Volume \\?\Volume{8f71ce79-bf4d-4cf5-9912-51e0b7ceba89} (\Device\HarddiskVolume39) is healthy.  No action is needed.
Information	12/9/2015 1:42:33 PM	Microsoft-Windows-Ntfs	98	None	Volume \\?\Volume{0d07cc6f-1601-4180-b5d7-649c8e3fec74} (\Device\HarddiskVolume79) is healthy.  No action is needed.
Information	12/9/2015 1:42:32 PM	Microsoft-Windows-Ntfs	98	None	Volume \\?\Volume{df2fbf69-b023-4ec3-a0fe-0310ca5484c6} (\Device\HarddiskVolume87) is healthy.  No action is needed.
Information	12/9/2015 1:42:32 PM	Microsoft-Windows-Ntfs	98	None	Volume \\?\Volume{593d710b-5728-45c9-a61a-e8f3de26eae2} (\Device\HarddiskVolume49) is healthy.  No action is needed.
Information	12/9/2015 1:42:32 PM	Microsoft-Windows-Ntfs	98	None	Volume \\?\Volume{729b2d84-1193-4625-9c24-c482044db076} (\Device\HarddiskVolume51) is healthy.  No action is needed.
Information	12/9/2015 1:42:31 PM	Microsoft-Windows-Ntfs	98	None	Volume \\?\Volume{d0e055e5-4567-4371-9e67-7184f8d609b0} (\Device\HarddiskVolume35) is healthy.  No action is needed.
Information	12/9/2015 1:42:30 PM	Microsoft-Windows-Ntfs	98	None	Volume \\?\Volume{7f056d30-b74c-4771-9f3b-feeba85c6786} (\Device\HarddiskVolume71) is healthy.  No action is needed.
Information	12/9/2015 1:42:12 PM	Microsoft-Windows-Ntfs	98	None	Volume \\?\Volume{2417d2ce-e5f0-4ccb-9952-0cdc2b905086} (\Device\HarddiskVolume73) is healthy.  No action is needed.
Information	12/9/2015 1:41:34 PM	Microsoft-Windows-Ntfs	98	None	Volume \\?\Volume{6798d74d-ce99-4746-8658-554efe2bb4d0} (\Device\HarddiskVolume41) is healthy.  No action is needed.
Information	12/9/2015 1:40:55 PM	Microsoft-Windows-Ntfs	98	None	Volume \\?\Volume{454715f7-3957-4358-98d5-0150b6f9c15d} (\Device\HarddiskVolume31) is healthy.  No action is needed.
Information	12/9/2015 1:40:44 PM	Microsoft-Windows-Ntfs	98	None	Volume \\?\Volume{456966bd-729e-4b43-bc2e-2f06682bb655} (\Device\HarddiskVolume77) is healthy.  No action is needed.
Information	12/9/2015 1:40:07 PM	Microsoft-Windows-Ntfs	98	None	Volume F: (\Device\HarddiskVolume7) is healthy.  No action is needed.
Information	12/9/2015 1:40:06 PM	Microsoft-Windows-Ntfs	98	None	Volume \\?\Volume{2e52d4ad-cb52-4f6d-b088-e899e97a6533} (\Device\HarddiskVolume44) is healthy.  No action is needed.
Information	12/9/2015 1:39:38 PM	Microsoft-Windows-Ntfs	98	None	Volume T: (\Device\HarddiskVolume89) is healthy.  No action is needed.
Information	12/9/2015 1:39:33 PM	Microsoft-Windows-Ntfs	98	None	Volume \\?\Volume{a4e5ff01-af34-4c7e-98c3-7c75de722f81} (\Device\HarddiskVolume15) is healthy.  No action is needed.
Information	12/9/2015 1:39:27 PM	Microsoft-Windows-Ntfs	98	None	Volume \\?\Volume{1f87331b-f3be-4bb1-a4b3-fda1fc37fadf} (\Device\HarddiskVolume23) is healthy.  No action is needed.
Information	12/9/2015 1:39:02 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 35 in group 7 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:39:02 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 33 in group 7 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:39:02 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 31 in group 7 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:39:01 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 29 in group 7 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:39:01 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 27 in group 7 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:39:01 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 25 in group 7 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:39:01 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 23 in group 7 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:39:01 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 21 in group 7 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:39:01 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 19 in group 7 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:39:01 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 17 in group 7 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:39:01 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 15 in group 7 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:39:01 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 13 in group 7 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:39:00 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 11 in group 7 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:39:00 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 9 in group 7 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:39:00 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 7 in group 7 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:39:00 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 5 in group 7 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:39:00 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 3 in group 7 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:39:00 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 1 in group 7 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:39:00 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 34 in group 7 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:39:00 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 32 in group 7 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:39:00 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 30 in group 7 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:59 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 28 in group 7 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:59 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 26 in group 7 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:59 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 24 in group 7 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:59 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 22 in group 7 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:59 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 20 in group 7 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:59 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 18 in group 7 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:59 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 16 in group 7 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:59 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 14 in group 7 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:58 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 12 in group 7 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:58 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 10 in group 7 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:58 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 8 in group 7 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:58 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 6 in group 7 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:58 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 4 in group 7 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:58 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 2 in group 7 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:58 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 0 in group 7 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:58 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 35 in group 6 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:58 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 33 in group 6 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:57 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 31 in group 6 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:57 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 29 in group 6 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:57 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 27 in group 6 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:57 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 25 in group 6 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:57 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 23 in group 6 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:57 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 21 in group 6 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:57 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 19 in group 6 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:57 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 17 in group 6 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:56 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 15 in group 6 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:56 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 13 in group 6 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:56 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 11 in group 6 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:56 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 9 in group 6 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:56 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 7 in group 6 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:56 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 5 in group 6 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:56 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 3 in group 6 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:56 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 1 in group 6 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:56 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 34 in group 6 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:55 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 32 in group 6 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:55 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 30 in group 6 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:55 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 28 in group 6 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:55 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 26 in group 6 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:55 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 24 in group 6 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:55 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 22 in group 6 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:55 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 20 in group 6 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:55 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 18 in group 6 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:55 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 16 in group 6 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:55 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 14 in group 6 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:55 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 12 in group 6 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:54 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 10 in group 6 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:54 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 8 in group 6 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:54 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 6 in group 6 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:54 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 4 in group 6 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:54 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 2 in group 6 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:54 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 0 in group 6 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:54 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 35 in group 5 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:54 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 33 in group 5 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:54 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 31 in group 5 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:53 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 29 in group 5 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:53 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 27 in group 5 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:53 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 25 in group 5 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:53 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 23 in group 5 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:53 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 21 in group 5 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:53 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 19 in group 5 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:53 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 17 in group 5 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:53 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 15 in group 5 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:53 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 13 in group 5 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:52 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 11 in group 5 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:52 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 9 in group 5 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:52 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 7 in group 5 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:52 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 5 in group 5 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:52 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 3 in group 5 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:52 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 1 in group 5 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:52 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 34 in group 5 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:52 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 32 in group 5 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:52 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 30 in group 5 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:51 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 28 in group 5 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:51 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 26 in group 5 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:51 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 24 in group 5 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:51 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 22 in group 5 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:51 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 20 in group 5 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:51 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 18 in group 5 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:51 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 16 in group 5 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:51 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 14 in group 5 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:51 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 12 in group 5 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:51 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 10 in group 5 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:50 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 8 in group 5 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:50 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 6 in group 5 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:50 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 4 in group 5 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:50 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 2 in group 5 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:50 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 0 in group 5 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:50 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 35 in group 4 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:50 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 33 in group 4 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:50 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 31 in group 4 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:49 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 29 in group 4 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:49 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 27 in group 4 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:49 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 25 in group 4 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:49 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 23 in group 4 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:49 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 21 in group 4 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:49 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 19 in group 4 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:49 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 17 in group 4 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:49 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 15 in group 4 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:49 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 13 in group 4 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:48 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 11 in group 4 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:48 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 9 in group 4 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:48 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 7 in group 4 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:48 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 5 in group 4 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:48 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 3 in group 4 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:48 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 1 in group 4 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:48 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 34 in group 4 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:48 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 32 in group 4 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:48 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 30 in group 4 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:48 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 28 in group 4 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:47 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 26 in group 4 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:47 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 24 in group 4 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:47 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 22 in group 4 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:47 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 20 in group 4 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:47 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 18 in group 4 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:47 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 16 in group 4 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:47 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 14 in group 4 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:47 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 12 in group 4 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:47 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 10 in group 4 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:46 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 8 in group 4 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:46 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 6 in group 4 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:46 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 4 in group 4 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:46 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 2 in group 4 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:46 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 0 in group 4 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:46 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 35 in group 3 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:46 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 33 in group 3 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:46 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 31 in group 3 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:46 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 29 in group 3 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:46 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 27 in group 3 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:46 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 25 in group 3 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:45 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 23 in group 3 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:45 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 21 in group 3 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:45 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 19 in group 3 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:45 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 17 in group 3 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:45 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 15 in group 3 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:45 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 13 in group 3 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:45 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 11 in group 3 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:45 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 9 in group 3 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:45 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 7 in group 3 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:44 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 5 in group 3 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:44 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 3 in group 3 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:44 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 1 in group 3 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:44 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 34 in group 3 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:44 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 32 in group 3 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:44 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 30 in group 3 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:44 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 28 in group 3 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:44 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 26 in group 3 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:44 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 24 in group 3 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:44 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 22 in group 3 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:43 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 20 in group 3 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:43 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 18 in group 3 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:43 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 16 in group 3 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:43 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 14 in group 3 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:43 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 12 in group 3 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:43 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 10 in group 3 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:43 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 8 in group 3 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:43 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 6 in group 3 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:43 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 4 in group 3 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:43 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 2 in group 3 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:43 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 0 in group 3 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:42 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 35 in group 2 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:42 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 33 in group 2 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:42 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 31 in group 2 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:42 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 29 in group 2 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:42 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 27 in group 2 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:42 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 25 in group 2 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:42 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 23 in group 2 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:42 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 21 in group 2 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:41 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 19 in group 2 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:41 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 17 in group 2 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:41 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 15 in group 2 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:41 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 13 in group 2 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:41 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 11 in group 2 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:41 PM	ixgbt	31	None	"Intel(R) Ethernet Converged Network Ad... [225,0,1]
 Network link has been established at 10Gbps full duplex.
"
Information	12/9/2015 1:38:41 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 9 in group 2 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:41 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 7 in group 2 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:41 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 5 in group 2 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:41 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 3 in group 2 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:41 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 1 in group 2 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:40 PM	ixgbt	31	None	"Intel(R) Ethernet Converged Network Ad... [161,0,1]
 Network link has been established at 10Gbps full duplex.
"
Information	12/9/2015 1:38:40 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 34 in group 2 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:40 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 32 in group 2 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:40 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 30 in group 2 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:40 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 28 in group 2 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:40 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 26 in group 2 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:40 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 24 in group 2 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:40 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 22 in group 2 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:40 PM	ixgbt	31	None	"Intel(R) Ethernet Converged Network Ada... [65,0,1]
 Network link has been established at 10Gbps full duplex.
"
Information	12/9/2015 1:38:40 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 20 in group 2 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:40 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 18 in group 2 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:40 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 16 in group 2 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:40 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 14 in group 2 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:39 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 12 in group 2 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:39 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 10 in group 2 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:39 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 8 in group 2 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:39 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 6 in group 2 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:39 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 4 in group 2 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:39 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 2 in group 2 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:39 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 0 in group 2 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:39 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 35 in group 1 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:39 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 33 in group 1 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:39 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 31 in group 1 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:38 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 29 in group 1 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:38 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 27 in group 1 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:38 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 25 in group 1 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:38 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 23 in group 1 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:38 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 21 in group 1 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:38 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 19 in group 1 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:38 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 17 in group 1 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:38 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 15 in group 1 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:38 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 13 in group 1 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:38 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 11 in group 1 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:37 PM	ixgbt	31	None	"Intel(R) Ethernet Controller X540-AT2 #3
 Network link has been established at 10Gbps full duplex.
"
Information	12/9/2015 1:38:37 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 9 in group 1 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:37 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 7 in group 1 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:37 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 5 in group 1 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:37 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 3 in group 1 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:37 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 1 in group 1 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Warning	12/9/2015 1:38:37 PM	ixgbt	27	None	"Intel(R) Ethernet Converged Network Ad... [225,0,1]
 Network link is disconnected.
"
Information	12/9/2015 1:38:37 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 34 in group 1 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:37 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 32 in group 1 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:37 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 30 in group 1 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:37 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 28 in group 1 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:37 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 26 in group 1 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Warning	12/9/2015 1:38:36 PM	ixgbt	27	None	"Intel(R) Ethernet Converged Network Ad... [161,0,1]
 Network link is disconnected.
"
Information	12/9/2015 1:38:36 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 24 in group 1 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:36 PM	ixgbt	32	None	"Intel(R) Ethernet Controller X540-AT2 #4
 Network link has been established at 1Gbps full duplex.
"
Information	12/9/2015 1:38:36 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 22 in group 1 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:36 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 20 in group 1 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:36 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 18 in group 1 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:36 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 16 in group 1 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:36 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 14 in group 1 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:36 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 12 in group 1 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:36 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 10 in group 1 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Warning	12/9/2015 1:38:36 PM	ixgbt	27	None	"Intel(R) Ethernet Converged Network Ada... [65,0,1]
 Network link is disconnected.
"
Information	12/9/2015 1:38:36 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 8 in group 1 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:36 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 6 in group 1 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:35 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 4 in group 1 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:35 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 2 in group 1 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:35 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 0 in group 1 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:35 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 35 in group 0 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:35 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 33 in group 0 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:35 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 31 in group 0 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:35 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 29 in group 0 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:35 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 27 in group 0 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:35 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 25 in group 0 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:35 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 23 in group 0 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:34 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 21 in group 0 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:34 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 19 in group 0 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Warning	12/9/2015 1:38:34 PM	ixgbt	27	None	"Intel(R) Ethernet Controller X540-AT2 #4
 Network link is disconnected.
"
Information	12/9/2015 1:38:34 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 17 in group 0 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:34 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 15 in group 0 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:34 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 13 in group 0 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:34 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 11 in group 0 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:34 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 9 in group 0 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:34 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 7 in group 0 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:33 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 5 in group 0 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Warning	12/9/2015 1:38:33 PM	ixgbt	27	None	"Intel(R) Ethernet Controller X540-AT2 #3
 Network link is disconnected.
"
Information	12/9/2015 1:38:33 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 3 in group 0 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:33 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 1 in group 0 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:33 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 34 in group 0 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:33 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 32 in group 0 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:33 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 30 in group 0 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:33 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 28 in group 0 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:33 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 26 in group 0 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:33 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 24 in group 0 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:33 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 22 in group 0 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:33 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 20 in group 0 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:32 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 18 in group 0 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:32 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 16 in group 0 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:32 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 14 in group 0 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:32 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 12 in group 0 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:32 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 10 in group 0 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:32 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 8 in group 0 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:32 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 6 in group 0 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:32 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 4 in group 0 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:32 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 2 in group 0 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:32 PM	Microsoft-Windows-Kernel-Processor-Power	55	(47)	"Processor 0 in group 0 exposes the following power management capabilities:

Idle state type: ACPI Idle (C) States (3 state(s))

Performance state type: ACPI Performance (P) / Throttle (T) States
Nominal Frequency (MHz): 2501
Maximum performance percentage: 100
Minimum performance percentage: 47
Minimum throttle percentage: 47"
Information	12/9/2015 1:38:05 PM	Microsoft-Windows-FilterManager	6	None	File System Filter 'npsvctrig' (6.3, ‎2013‎-‎08‎-‎22T06:38:22.000000000Z) has successfully loaded and registered with Filter Manager.
Information	12/9/2015 1:37:16 PM	Microsoft-Windows-Ntfs	98	None	Volume C: (\Device\HarddiskVolume4) is healthy.  No action is needed.
Information	12/9/2015 1:35:33 PM	TPM	24	None	The Trusted Platform Module (TPM) status: Enabled and Active.
Information	12/9/2015 1:34:15 PM	Microsoft-Windows-Kernel-Boot	27	None	The boot type was 0x0.
Information	12/9/2015 1:34:15 PM	Microsoft-Windows-Kernel-Boot	20	None	The last shutdown's success status was true. The last boot's success status was true.
Information	12/9/2015 1:34:15 PM	Microsoft-Windows-Kernel-Boot	32	None	The bootmgr spent 0 ms waiting for user input.
Information	12/9/2015 1:34:15 PM	Microsoft-Windows-Kernel-Boot	18	None	There are 0x1 boot options on this system.
Information	12/9/2015 1:34:15 PM	Microsoft-Windows-Kernel-General	12	None	The operating system started at system time ‎2015‎-‎12‎-‎09T18:32:45.490308600Z.
Information	12/9/2015 12:57:50 PM	Microsoft-Windows-Kernel-General	13	None	The operating system is shutting down at system time ‎2015‎-‎12‎-‎09T17:57:50.974957300Z.
Information	12/9/2015 12:57:48 PM	Microsoft-Windows-Kernel-Power	109	(103)	The kernel power manager has initiated a shutdown transition.
Information	12/9/2015 12:57:48 PM	Microsoft-Windows-Kernel-Power	109	(103)	The kernel power manager has initiated a shutdown transition.
Information	12/9/2015 12:57:48 PM	Service Control Manager	7036	None	The Cryptographic Services service entered the stopped state.
Information	12/9/2015 12:57:48 PM	Service Control Manager	7036	None	The Remote Desktop Services service entered the stopped state.
Information	12/9/2015 12:57:48 PM	Service Control Manager	7036	None	The Windows Font Cache Service service entered the stopped state.
Information	12/9/2015 12:57:48 PM	Service Control Manager	7036	None	The Device Setup Manager service entered the stopped state.
Information	12/9/2015 12:57:48 PM	Service Control Manager	7036	None	The Task Scheduler service entered the stopped state.
Information	12/9/2015 12:57:48 PM	Service Control Manager	7036	None	The IKE and AuthIP IPsec Keying Modules service entered the stopped state.
Information	12/9/2015 12:57:48 PM	Service Control Manager	7036	None	The Windows Connection Manager service entered the stopped state.
Information	12/9/2015 12:57:48 PM	Service Control Manager	7036	None	The Distributed Transaction Coordinator service entered the stopped state.
Information	12/9/2015 12:57:48 PM	Service Control Manager	7036	None	The Windows Remote Management (WS-Management) service entered the stopped state.
Information	12/9/2015 12:57:48 PM	Service Control Manager	7036	None	The Windows Event Log service entered the stopped state.
Information	12/9/2015 12:57:48 PM	Service Control Manager	7036	None	The Windows Management Instrumentation service entered the stopped state.
Information	12/9/2015 12:57:48 PM	Service Control Manager	7036	None	The IPsec Policy Agent service entered the stopped state.
Information	12/9/2015 1:42:48 PM	EventLog	6013	None	The system uptime is 603 seconds.
Information	12/9/2015 1:42:48 PM	EventLog	6005	None	The Event log service was started.
Information	12/9/2015 1:42:48 PM	EventLog	6009	None	Microsoft (R) Windows (R) 6.03. 9600  Multiprocessor Free.
Information	12/9/2015 12:57:48 PM	Service Control Manager	7036	None	The User Profile Service service entered the stopped state.
Information	12/9/2015 12:57:48 PM	Service Control Manager	7036	None	The DHCP Client service entered the stopped state.
Information	12/9/2015 12:57:48 PM	Microsoft-Windows-Dhcp-Client	50037	Service State Event	DHCPv4 client service is stopped. ShutDown Flag value is 1
Information	12/9/2015 12:57:48 PM	Microsoft-Windows-DHCPv6-Client	51047	Service State Event	DHCPv6 client service is stopped. ShutDown Flag value is 1
Information	12/9/2015 12:57:48 PM	Service Control Manager	7036	None	The SQL Server VSS Writer service entered the stopped state.
Information	12/9/2015 12:57:48 PM	Service Control Manager	7036	None	The Diagnostic Policy Service service entered the stopped state.
Information	12/9/2015 12:57:48 PM	Service Control Manager	7036	None	The Certificate Propagation service entered the stopped state.
Information	12/9/2015 12:57:48 PM	Service Control Manager	7036	None	The Distributed Link Tracking Client service entered the stopped state.
Information	12/9/2015 12:57:48 PM	Service Control Manager	7036	None	The Remote Desktop Services UserMode Port Redirector service entered the stopped state.
Information	12/9/2015 12:57:48 PM	Service Control Manager	7036	None	The Plug and Play service entered the stopped state.
Information	12/9/2015 12:57:48 PM	Service Control Manager	7036	None	The User Access Logging Service service entered the stopped state.
Information	12/9/2015 12:57:48 PM	EventLog	6006	None	The Event log service was stopped.
Warning	12/9/2015 12:57:48 PM	Microsoft-Windows-WinRM	10149	None	"The WinRM service is not listening for WS-Management requests. 

 User Action 
 If you did not intentionally stop the service, use the following command to see the WinRM configuration: 

 winrm enumerate winrm/config/listener"
Information	12/9/2015 12:57:48 PM	Service Control Manager	7036	None	The Group Policy Client service entered the stopped state.
Information	12/9/2015 12:57:48 PM	Microsoft-Windows-Winlogon	7002	(1102)	User Logoff Notification for Customer Experience Improvement Program
Information	12/9/2015 12:57:48 PM	User32	1074	None	"The process C:\Windows\system32\winlogon.exe (IBMSERV) has initiated the power off of computer IBMSERV on behalf of user IBMSERV\Administrator for the following reason: No title for this reason could be found
 Reason Code: 0x500ff
 Shutdown Type: power off
 Comment: "
Information	12/9/2015 12:57:47 PM	Service Control Manager	7036	None	The WinHTTP Web Proxy Auto-Discovery Service service entered the running state.
Information	12/9/2015 12:57:47 PM	User32	1074	None	"The process Explorer.EXE has initiated the power off of computer IBMSERV on behalf of user IBMSERV\Administrator for the following reason: Other (Unplanned)
 Reason Code: 0x0
 Shutdown Type: power off
 Comment: "
Information	12/9/2015 12:55:29 PM	Microsoft-Windows-Eventlog	104	Log clear	The System log file was cleared.
